,Model##other##,Description##other##,Height##Length##inches,Default Placement Height##Length##Inches,With Cutouts##other##,Right Side Without Cutouts##other##,Right Side With Cutouts##other##,Left Side Without Cutouts##other##,Left Side With Cutouts##other##,Right Side##other##,Left Side##other##,CTRL Masking##other##,CTRL Masking 2##other##,CTRL Masking 3##other##,PosOpt##Other##
"24""H Left W/Cutouts",TW400.24LC,Close-out Side Lft cutout(s)for wall rail  24H,22.74,41.925,1,0,0,0,1,0,1,0,1,0,0
"24""H Left No Cutouts",TW400.24LN,Close-out Side Lft no cutout(s)for wall rail  24H,22.74,41.925,0,0,0,1,0,0,1,0,0,1,0
"24""H Right W/Cutouts",TW400.24RC,Close-out Side Rt cutout(s)for wall rail  24H,22.74,41.925,1,0,1,0,0,1,0,0,1,0,0
"24""H Right No Cutouts",TW400.24RN,Close-out Side Rt no cutout(s)for wall rail  24H,22.74,41.925,0,1,0,0,0,1,0,0,0,1,0
"64""H Left W/Cutouts",TW400.64LC,Close-out Side Lft cutout(s)for wall rail  64H,62.645,81.425,1,0,0,0,1,0,1,1,0,0,0
"64""H Left  No Cutouts",TW400.64LN,Close-out Side Lft no cutout(s)for wall rail  64H,62.645,81.425,0,0,0,1,0,0,1,0,0,1,0
"64""H Right W/Cutouts",TW400.64RC,Close-out Side Rt cutout(s)for wall rail  64H,62.645,81.425,1,0,1,0,0,1,0,1,0,0,0
"64""H Right No Cutouts",TW400.64RN,Close-out Side Rt no cutout(s)for wall rail  64H,62.645,81.425,0,1,0,0,0,1,0,0,0,1,0
"89""H Left W/Cutouts",TW400.89LC,Close-out Side Lft cutout(s)for wall rail  89H,88.835,81.425,1,0,0,0,1,0,1,1,0,0,1
"89""H Left  No Cutouts",TW400.89LN,Close-out Side Lft no cutout(s)for wall rail  89H,88.835,81.425,0,0,0,1,0,0,1,0,0,1,1
"89""H Right W/Cutouts",TW400.89RC,Close-out Side Rt cutout(s)for wall rail  89H,88.835,81.425,1,0,1,0,0,1,0,1,0,0,1
"89""H Right No Cutouts",TW400.89RN,Close-out Side Rt no cutout(s)for wall rail  89H,88.835,81.425,0,1,0,0,0,1,0,0,0,1,1
"89""H Left W/Cutouts Use W/64H Sloped Cab Top",TW400.89LC,Close-out Side Lft cutout(s)for wall rail  89H,63.6448,81.425,1,0,0,0,1,0,1,1,0,0,0
"89""H Left  No Cutouts Use W/64H Sloped Cab Top",TW400.89LN,Close-out Side Lft no cutout(s)for wall rail  89H,63.6448,81.425,0,0,0,1,0,0,1,0,0,1,0
"89""H Right W/Cutouts Use W/64H Sloped Cab Top",TW400.89RC,Close-out Side Rt cutout(s)for wall rail  89H,63.6448,81.425,1,0,1,0,0,1,0,1,0,0,0
"89""H Right No Cutouts Use W/64H Sloped Cab Top",TW400.89RN,Close-out Side Rt no cutout(s)for wall rail  89H,63.6448,81.425,0,1,0,0,0,1,0,0,0,1,0
