,Model##Other##,Description##Other##,Tag##Other##,Width##Length##Inches,Left##Other##
"36""W Left-hand Swing Lock Set Reverse Bevel",E1119.36LWR,Door Frame With Door and Lever Left-hand Swing Lock Set Reverse Bevel 36W,86/36,36,1
"36""W Left-hand Swing Lock Set Standard Bevel",E1119.36LWS,Door Frame With Door and Lever Left-hand Swing Lock Set Standard Bevel 36W,86/36,36,1
"36""W Left-hand Swing No Set Reverse Bevel",E1119.36LOR,Door Frame With Door and Lever Left-hand Swing No Set Reverse Bevel 36W,86/36,36,1
"36""W Left-hand Swing No Set Standard Bevel",E1119.36LOS,Door Frame With Door and Lever Left-hand Swing No Set Standard Bevel 36W,86/36,36,1
"36""W Left-hand Swing Passage Set Reverse Bevel",E1119.36LNR,Door Frame With Door and Lever Left-hand Swing Passage Set Reverse Bevel 36W,86/36,36,1
"36""W Left-hand Swing Passage Set Standard Bevel",E1119.36LNS,Door Frame With Door and Lever Left-hand Swing Passage Set Standard Bevel 36W,86/36,36,1
"36""W Right-hand Swing Lock Set Reverse Bevel",E1119.36RWR,Door Frame With Door and Lever Right-hand Swing Lock Set Reverse Bevel 36W,86/36,36,0
"36""W Right-hand Swing Lock Set Standard Bevel",E1119.36RWS,Door Frame With Door and Lever Right-hand Swing Lock Set Standard Bevel 36W,86/36,36,0
"36""W Right-hand Swing No Set Reverse Bevel",E1119.36ROR,Door Frame With Door and Lever Right-hand Swing No Set Reverse Bevel 36W,86/36,36,0
"36""W Right-hand Swing No Set Standard Bevel",E1119.36ROS,Door Frame With Door and Lever Right-hand Swing No Set Standard Bevel 36W,86/36,36,0
"36""W Right-hand Swing Passage Set Reverse Bevel",E1119.36RNR,Door Frame With Door and Lever Right-hand Swing Passage Set Reverse Bevel 36W,86/36,36,0
"36""W Right-hand Swing Passage Set Standard Bevel",E1119.36RNS,Door Frame With Door and Lever Right-hand Swing Passage Set Standard Bevel 36W,86/36,36,0
"42""W Left-hand Swing Lock Set Reverse Bevel",E1119.42LWR,Door Frame With Door and Lever Left-hand Swing Lock Set Reverse Bevel 42W,86/42,42,1
"42""W Left-hand Swing Lock Set Standard Bevel",E1119.42LWS,Door Frame With Door and Lever Left-hand Swing Lock Set Standard Bevel 42W,86/42,42,1
"42""W Left-hand Swing No Set Reverse Bevel",E1119.42LOR,Door Frame With Door and Lever Left-hand Swing No Set Reverse Bevel 42W,86/42,42,1
"42""W Left-hand Swing No Set Standard Bevel",E1119.42LOS,Door Frame With Door and Lever Left-hand Swing No Set Standard Bevel 42W,86/42,42,1
"42""W Left-hand Swing Passage Set Reverse Bevel",E1119.42LNR,Door Frame With Door and Lever Left-hand Swing Passage Set Reverse Bevel 42W,86/42,42,1
"42""W Left-hand Swing Passage Set Standard Bevel",E1119.42LNS,Door Frame With Door and Lever Left-hand Swing Passage Set Standard Bevel 42W,86/42,42,1
"42""W Right-hand Swing Lock Set Reverse Bevel",E1119.42RWR,Door Frame With Door and Lever Right-hand Swing Lock Set Reverse Bevel 42W,86/42,42,0
"42""W Right-hand Swing Lock Set Standard Bevel",E1119.42RWS,Door Frame With Door and Lever Right-hand Swing Lock Set Standard Bevel 42W,86/42,42,0
"42""W Right-hand Swing No Set Reverse Bevel",E1119.42ROR,Door Frame With Door and Lever Right-hand Swing No Set Reverse Bevel 42W,86/42,42,0
"42""W Right-hand Swing No Set Standard Bevel",E1119.42ROS,Door Frame With Door and Lever Right-hand Swing No Set Standard Bevel 42W,86/42,42,0
"42""W Right-hand Swing Passage Set Reverse Bevel",E1119.42RNR,Door Frame With Door and Lever Right-hand Swing Passage Set Reverse Bevel 42W,86/42,42,0
"42""W Right-hand Swing Passage Set Standard Bevel",E1119.42RNS,Door Frame With Door and Lever Right-hand Swing Passage Set Standard Bevel 42W,86/42,42,0
