,Model##Other##,Description##Other##,Tag##Other##,Frame Width##Length##Inches,Socket Visibility Exterior##Other##,Communication Port Exterior##Other##,Electrical Connector##Other##,Connector Description##Other##,Chicago##Other##,Chicago Two Recep##Other##
24W 2 Receps 1 Comm Port,E1264.24J,Side Cover Grooved 2 Receps 1 Comm Port 24W,J,24,1,1,1,Electrical Connector Enabled,0,0
30W 2 Receps 1 Comm Port,E1264.30J,Side Cover Grooved 2 Receps 1 Comm Port 30W,J,30,1,1,1,Electrical Connector Enabled,0,0
36W 2 Receps 1 Comm Port,E1264.36J,Side Cover Grooved 2 Receps 1 Comm Port 36W,J,36,1,1,1,Electrical Connector Enabled,0,0
42W 2 Receps 1 Comm Port,E1264.42J,Side Cover Grooved 2 Receps 1 Comm Port 42W,J,42,1,1,1,Electrical Connector Enabled,0,0
48W 2 Receps 1 Comm Port,E1264.48J,Side Cover Grooved 2 Receps 1 Comm Port 48W,J,48,1,1,1,Electrical Connector Enabled,0,0
24W 1 Recep Chi,E1264.24R,Side Cover Grooved 1 Recep Chi 24W,R,24,0,0,0,Electrical Connector Enabled,1,0
30W 1 Recep Chi,E1264.30R,Side Cover Grooved 1 Recep Chi 30W,R,30,0,0,0,Electrical Connector Enabled,1,0
36W 2 Receps Chi,E1264.36R,Side Cover Grooved 2 Receps Chi 36W,R,36,0,0,0,Electrical Connector Enabled,0,1
42W 2 Receps Chi,E1264.42R,Side Cover Grooved 2 Receps Chi 42W,R,42,0,0,0,Electrical Connector Enabled,0,1
48W 2 Receps Chi,E1264.48R,Side Cover Grooved 2 Receps Chi 48W,R,48,0,0,0,Electrical Connector Enabled,0,1
18W No Receps,E1264.18N,Side Cover Grooved No Receps 18W,N,18,0,0,0,Electrical Connector Enabled,0,0
24W No Receps,E1264.24N,Side Cover Grooved No Receps 24W,N,24,0,0,0,Electrical Connector Enabled,0,0
30W No Receps,E1264.30N,Side Cover Grooved No Receps 30W,N,30,0,0,0,Electrical Connector Enabled,0,0
36W No Receps,E1264.36N,Side Cover Grooved No Receps 36W,N,36,0,0,0,Electrical Connector Enabled,0,0
42W No Receps,E1264.42N,Side Cover Grooved No Receps 42W,N,42,0,0,0,Electrical Connector Enabled,0,0
48W No Receps,E1264.48N,Side Cover Grooved No Receps 48W,N,48,0,0,0,Electrical Connector Enabled,0,0
