,Model##Other##,Description##Other##,Panel Height##Length##Inches,Panel Width##Length##Inches,Socket Visibility Interior Left##Other##,Socket Visibility Interior Right##Other##,Socket Visibility Exterior Right##Other##,Socket Visibility Exterior Left##Other##,Communication Port Exterior##Other##,Communication Port Interior##Other##,Electrical Connector##Other##,Connector Description##Other##,Tag##Other##,Powered##Other##,Communication Socket Location##Length##Inches,Electrical Socket Location##Length##Inches,Electrical Socket 2 Location##Length##Inches
"53""H x 24""W-G",A8164.5324G,Panel Partial-Glazed Thin Base 4-Circ W/Rcp & Com Pt Lc 53H 24W,53,24,1,0,0,1,1,1,1,Electrical Connector Enabled,53/24G,1,4.125,11.91,11.91
"53""H x 30""W-G",A8164.5330G,Panel Partial-Glazed Thin Base 4-Circ W/Rcp & Com Pt Lc 53H 30W,53,30,1,1,1,1,1,1,1,Electrical Connector Enabled,53/30G,1,13.125,9.09,9.09
"53""H x 36""W-G",A8164.5336G,Panel Partial-Glazed Thin Base 4-Circ W/Rcp & Com Pt Lc 53H 36W,53,36,1,1,1,1,1,1,1,Electrical Connector Enabled,53/36G,1,16.125,9.09,9.09
"53""H x 48""W-G",A8164.5348G,Panel Partial-Glazed Thin Base 4-Circ W/Rcp & Com Pt Lc 53H 48W,53,48,1,1,1,1,1,1,1,Electrical Connector Enabled,53/48G,1,22.125,9.09,9.09
"67""H x 24""W-G",A8164.6724G,Panel Partial-Glazed Thin Base 4-Circ W/Rcp & Com Pt Lc 67H 24W,67,24,1,0,0,1,1,1,1,Electrical Connector Enabled,67/24G,1,4.125,11.91,11.91
"67""H x 30""W-G",A8164.6730G,Panel Partial-Glazed Thin Base 4-Circ W/Rcp & Com Pt Lc 67H 30W,67,30,1,1,1,1,1,1,1,Electrical Connector Enabled,67/30G,1,13.125,9.09,9.09
"67""H x 36""W-G",A8164.6736G,Panel Partial-Glazed Thin Base 4-Circ W/Rcp & Com Pt Lc 67H 36W,67,36,1,1,1,1,1,1,1,Electrical Connector Enabled,67/36G,1,16.125,9.09,9.09
"67""H x 48""W-G",A8164.6748G,Panel Partial-Glazed Thin Base 4-Circ W/Rcp & Com Pt Lc 67H 48W,67,48,1,1,1,1,1,1,1,Electrical Connector Enabled,67/48G,1,22.125,9.09,9.09
"85""H x 24""W-G",A8164.8524G,Panel Partial-Glazed Thin Base 4-Circ W/Rcp & Com Pt Lc 85H 24W,85,24,1,0,0,1,1,1,1,Electrical Connector Enabled,85/24G,1,4.125,11.91,11.91
"85""H x 30""W-G",A8164.8530G,Panel Partial-Glazed Thin Base 4-Circ W/Rcp & Com Pt Lc 85H 30W,85,30,1,1,1,1,1,1,1,Electrical Connector Enabled,85/30G,1,13.125,9.09,9.09
"85""H x 36""W-G",A8164.8536G,Panel Partial-Glazed Thin Base 4-Circ W/Rcp & Com Pt Lc 85H 36W,85,36,1,1,1,1,1,1,1,Electrical Connector Enabled,85/36G,1,16.125,9.09,9.09
"85""H x 48""W-G",A8164.8548G,Panel Partial-Glazed Thin Base 4-Circ W/Rcp & Com Pt Lc 85H 48W,85,48,1,1,1,1,1,1,1,Electrical Connector Enabled,85/48G,1,22.125,9.09,9.09
"53""H x 24""W-N",A8164.5324N,Panel Partial-Glazed Thin Base Npwr 53H 24W,53,24,0,0,0,0,0,0,0,Electrical Connector Disabled,53/24N,0,4.125,11.91,11.91
"53""H x 30""W-N",A8164.5330N,Panel Partial-Glazed Thin Base Npwr 53H 30W,53,30,0,0,0,0,0,0,0,Electrical Connector Disabled,53/30N,0,13.125,9.09,9.09
"53""H x 36""W-N",A8164.5336N,Panel Partial-Glazed Thin Base Npwr 53H 36W,53,36,0,0,0,0,0,0,0,Electrical Connector Disabled,53/36N,0,16.125,9.09,9.09
"53""H x 48""W-N",A8164.5348N,Panel Partial-Glazed Thin Base Npwr 53H 48W,53,48,0,0,0,0,0,0,0,Electrical Connector Disabled,53/48N,0,22.125,9.09,9.09
"67""H x 24""W-N",A8164.6724N,Panel Partial-Glazed Thin Base Npwr 67H 24W,67,24,0,0,0,0,0,0,0,Electrical Connector Disabled,67/24N,0,4.125,11.91,11.91
"67""H x 30""W-N",A8164.6730N,Panel Partial-Glazed Thin Base Npwr 67H 30W,67,30,0,0,0,0,0,0,0,Electrical Connector Disabled,67/30N,0,13.125,9.09,9.09
"67""H x 36""W-N",A8164.6736N,Panel Partial-Glazed Thin Base Npwr 67H 36W,67,36,0,0,0,0,0,0,0,Electrical Connector Disabled,67/36N,0,16.125,9.09,9.09
"67""H x 48""W-N",A8164.6748N,Panel Partial-Glazed Thin Base Npwr 67H 48W,67,48,0,0,0,0,0,0,0,Electrical Connector Disabled,67/48N,0,22.125,9.09,9.09
"85""H x 24""W-N",A8164.8524N,Panel Partial-Glazed Thin Base Npwr 85H 24W,85,24,0,0,0,0,0,0,0,Electrical Connector Disabled,85/24N,0,4.125,11.91,11.91
"85""H x 30""W-N",A8164.8530N,Panel Partial-Glazed Thin Base Npwr 85H 30W,85,30,0,0,0,0,0,0,0,Electrical Connector Disabled,85/30N,0,13.125,9.09,9.09
"85""H x 36""W-N",A8164.8536N,Panel Partial-Glazed Thin Base Npwr 85H 36W,85,36,0,0,0,0,0,0,0,Electrical Connector Disabled,85/36N,0,16.125,9.09,9.09
"85""H x 48""W-N",A8164.8548N,Panel Partial-Glazed Thin Base Npwr 85H 48W,85,48,0,0,0,0,0,0,0,Electrical Connector Disabled,85/48N,0,22.125,9.09,9.09
"53""H x 24""W-J",A8164.5324J,Panel Partial-Glazed Thin Base Npwr W/Rcp & Com Pt Lc 53H 24W,53,24,1,0,0,1,1,1,0,Electrical Connector Disabled,53/24J,0,4.125,11.91,11.91
"53""H x 30""W-J",A8164.5330J,Panel Partial-Glazed Thin Base Npwr W/Rcp & Com Pt Lc 53H 30W,53,30,1,1,1,1,1,1,0,Electrical Connector Disabled,53/30J,0,13.125,9.09,9.09
"53""H x 36""W-J",A8164.5336J,Panel Partial-Glazed Thin Base Npwr W/Rcp & Com Pt Lc 53H 36W,53,36,1,1,1,1,1,1,0,Electrical Connector Disabled,53/36J,0,16.125,9.09,9.09
"53""H x 48""W-J",A8164.5348J,Panel Partial-Glazed Thin Base Npwr W/Rcp & Com Pt Lc 53H 48W,53,48,1,1,1,1,1,1,0,Electrical Connector Disabled,53/48J,0,22.125,9.09,9.09
"67""H x 24""W-J",A8164.6724J,Panel Partial-Glazed Thin Base Npwr W/Rcp & Com Pt Lc 67H 24W,67,24,1,0,0,1,1,1,0,Electrical Connector Disabled,67/24J,0,4.125,11.91,11.91
"67""H x 30""W-J",A8164.6730J,Panel Partial-Glazed Thin Base Npwr W/Rcp & Com Pt Lc 67H 30W,67,30,1,1,1,1,1,1,0,Electrical Connector Disabled,67/30J,0,13.125,9.09,9.09
"67""H x 36""W-J",A8164.6736J,Panel Partial-Glazed Thin Base Npwr W/Rcp & Com Pt Lc 67H 36W,67,36,1,1,1,1,1,1,0,Electrical Connector Disabled,67/36J,0,16.125,9.09,9.09
"67""H x 48""W-J",A8164.6748J,Panel Partial-Glazed Thin Base Npwr W/Rcp & Com Pt Lc 67H 48W,67,48,1,1,1,1,1,1,0,Electrical Connector Disabled,67/48J,0,22.125,9.09,9.09
"85""H x 24""W-J",A8164.8524J,Panel Partial-Glazed Thin Base Npwr W/Rcp & Com Pt Lc 85H 24W,85,24,1,0,0,1,1,1,0,Electrical Connector Disabled,85/24J,0,4.125,11.91,11.91
"85""H x 30""W-J",A8164.8530J,Panel Partial-Glazed Thin Base Npwr W/Rcp & Com Pt Lc 85H 30W,85,30,1,1,1,1,1,1,0,Electrical Connector Disabled,85/30J,0,13.125,9.09,9.09
"85""H x 36""W-J",A8164.8536J,Panel Partial-Glazed Thin Base Npwr W/Rcp & Com Pt Lc 85H 36W,85,36,1,1,1,1,1,1,0,Electrical Connector Disabled,85/36J,0,16.125,9.09,9.09
"85""H x 48""W-J",A8164.8548J,Panel Partial-Glazed Thin Base Npwr W/Rcp & Com Pt Lc 85H 48W,85,48,1,1,1,1,1,1,0,Electrical Connector Disabled,85/48J,0,22.125,9.09,9.09
"53""H x 24""W-R",A8164.5324R,Panel Partial-Glazed Thin Base Npwr W/Rcp Lc (Meets Chicago code) 53H 24W,53,24,1,0,0,1,1,1,0,Electrical Connector Disabled,53/24R,0,16.975,10.66,10.66
"53""H x 30""W-R",A8164.5330R,Panel Partial-Glazed Thin Base Npwr W/Rcp Lc (Meets Chicago code) 53H 30W,53,30,1,1,1,1,1,1,0,Electrical Connector Disabled,53/30R,0,21.375,13.66,13.66
"53""H x 36""W-R",A8164.5336R,Panel Partial-Glazed Thin Base Npwr W/Rcp Lc (Meets Chicago code) 53H 36W,53,36,1,1,1,1,1,1,0,Electrical Connector Disabled,53/36R,0,29.125,23.91,13.84
"53""H x 48""W-R",A8164.5348R,Panel Partial-Glazed Thin Base Npwr W/Rcp Lc (Meets Chicago code) 53H 48W,53,48,1,1,1,1,1,1,0,Electrical Connector Disabled,53/48R,0,35.125,29.91,19.84
"67""H x 24""W-R",A8164.6724R,Panel Partial-Glazed Thin Base Npwr W/Rcp Lc (Meets Chicago code) 67H 24W,67,24,1,0,0,1,1,1,0,Electrical Connector Disabled,67/24R,0,16.975,10.66,10.66
"67""H x 30""W-R",A8164.6730R,Panel Partial-Glazed Thin Base Npwr W/Rcp Lc (Meets Chicago code) 67H 30W,67,30,1,0,0,1,1,1,0,Electrical Connector Disabled,67/30R,0,21.375,13.66,13.66
"67""H x 36""W-R",A8164.6736R,Panel Partial-Glazed Thin Base Npwr W/Rcp Lc (Meets Chicago code) 67H 36W,67,36,1,1,1,1,1,1,0,Electrical Connector Disabled,67/36R,0,29.125,23.91,13.84
"67""H x 48""W-R",A8164.6748R,Panel Partial-Glazed Thin Base Npwr W/Rcp Lc (Meets Chicago code) 67H 48W,67,48,1,1,1,1,1,1,0,Electrical Connector Disabled,67/48R,0,35.125,29.91,19.84
"85""H x 24""W-R",A8164.8524R,Panel Partial-Glazed Thin Base Npwr W/Rcp Lc (Meets Chicago code) 85H 24W,85,24,1,0,0,1,1,1,0,Electrical Connector Disabled,85/24R,0,16.975,10.66,10.66
"85""H x 30""W-R",A8164.8530R,Panel Partial-Glazed Thin Base Npwr W/Rcp Lc (Meets Chicago code) 85H 30W,85,30,1,0,0,1,1,1,0,Electrical Connector Disabled,85/30R,0,21.375,13.66,13.66
"85""H x 36""W-R",A8164.8536R,Panel Partial-Glazed Thin Base Npwr W/Rcp Lc (Meets Chicago code) 85H 36W,85,36,1,1,1,1,1,1,0,Electrical Connector Disabled,85/36R,0,29.125,23.91,13.84
"85""H x 48""W-R",A8164.8548R,Panel Partial-Glazed Thin Base Npwr W/Rcp Lc (Meets Chicago code) 85H 48W,85,48,1,1,1,1,1,1,0,Electrical Connector Disabled,85/48R,0,35.125,29.91,19.84
