,Model##Other##,Description##Other##,Has Isolated Ground##Other##,3 Circuit##Other##,Letter##Other##,Controlled Distance##Length##Inches,Controlled##Other##
A,E1311.A,15 Amp Receptacle 4 Circuit  Duplex  Circuit A 6/Pkg,0,0,HermanMiller_Circuit_A : A,3.814,0
B,E1311.B,15 Amp Receptacle 4 Circuit  Duplex  Circuit B 6/Pkg,0,0,HermanMiller_Circuit_B : B,3.814,0
BI Isolated,E1311.BI,15 Amp Receptacle 4 Circuit  Duplex  Circuit B isolated ground 6/Pkg,1,0,HermanMiller_Circuit_B : B,0,0
C,E1311.C,15 Amp Receptacle 4 Circuit  Duplex  Circuit C 6/Pkg,0,0,HermanMiller_Circuit_C : C,3.814,0
CI Isolated,E1311.CI,15 Amp Receptacle 4 Circuit  Duplex  Circuit C isolated ground 6/Pkg,1,0,HermanMiller_Circuit_C : C,0,0
CI Isolated 3 Circuit,E1311.CS,16 Amp Receptacle 3 Circuit  Duplex  Circuit C isolated ground 6/Pkg,1,1,HermanMiller_Circuit_C : C,0,0
D Isolated,E1311.D,15 Amp Receptacle 4 Circuit  Duplex  Circuit D isolated ground 6/Pkg,1,0,HermanMiller_Circuit_D : D,0,0
DN,E1311.DN,15 Amp Receptacle 4 Circuit  Duplex  Circuit D 6/Pkg,0,0,HermanMiller_Circuit_D : D,3.814,0
A Controlled,E1311M.A,Controlled Receptacle 4 Circuit 15 Amp  Duplex  Circuit A 6/Pkg,0,0,HermanMiller_Circuit_A : A,0,1
B Controlled,E1311M.B,Controlled Receptacle 4 Circuit 15 Amp  Duplex  Circuit B 6/Pkg,0,0,HermanMiller_Circuit_B : B,0,1
BI Isolated Controlled,E1311M.BI,Controlled Receptacle 4 Circuit 15 Amp  Duplex  Circuit B isolated ground 6/Pkg,1,0,HermanMiller_Circuit_B : B,3.814,1
C Controlled,E1311M.C,Controlled Receptacle 4 Circuit 15 Amp  Duplex  Circuit C 6/Pkg,0,0,HermanMiller_Circuit_C : C,0,1
CI Isolated Controlled,E1311M.CI,Controlled Receptacle 4 Circuit 15 Amp  Duplex  Circuit C isolated ground 6/Pkg,1,0,HermanMiller_Circuit_C : C,3.814,1
D Isolated Controlled,E1311M.D,Controlled Receptacle 4 Circuit 15 Amp  Duplex  Circuit D isolated ground 6/Pkg,1,0,HermanMiller_Circuit_D : D,3.814,1
DN Controlled,E1311M.DN,Controlled Receptacle 4 Circuit 15 Amp  Duplex  Circuit D 6/Pkg,0,0,HermanMiller_Circuit_D : D,0,1
